Ⅰ.Specification
1) . Item No.:
     D350I
2). Power Rate:      500W - 3500W

3). Voltage:
     220V ~ 50Hz  

4). Temperature:
     60℃-240℃

Ⅱ. Importance


Please read carefully the following instructions before using the induction cooker.
1). Do not plug with wet hands in order to avoid getting electric shock.

2). Do not plug into a socket where several other appliances are plugged in.

3). Do not use if the power cord is damaged or the plug does not fit the socket safely.

4). Do not open the cooker to replace spare parts by yourself.

5). Do not use the cooker closed to flame or wet places.

6). Do not use where children can easily touch the cooker, or allow children to use the cooker by themselves.

7). Do not place on unstable surfaces.

8). Do not move the cooker together with a pot.

9). Do not heat a pot empty or overheat to avoid dry boiling.

10). Do not place metallic objects such as knives, forks, spoons, lids, cans, and aluminum foils on the concave disc.

11). Use the unit with sufficient space around it. Keep the front side and either right or left side of the unit clear.

12). Do not use the unit on carpet or tablecloth (vinyl) or any other low-heat-resistant article.

13). Do not place a sheet of paper between the pot or the pan and the unit. The paper may get burnt.

14). If the surface is cracked, switch off and take to the service center immediately.

15). Do not block air intake or exhaust vent.

16). Do not touch the concave disc right after removing the pot or the pan, as the concave disc will still be very hot.

17). Do not place the cooker close to the objects which are affected by magnet, such as: radios, televisions, automatic-banking cards or cassette tapes.

18). The power cord must be replaced by qualified technicians.
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The surface is liable to get hot during use.

20)  This appliance is not intended for use by persons (including children) with reduced physical, sensory or mental capabilities, or lack of experience and knowledge, unless they have been given supervision or  instruction concerning use of the appliance by a person responsible for their safety.

Warning: Children should be supervised to ensure that they do not play with the appliance.  

Ⅲ.How to Use
1). Please put suitable cookware onto the plate of induction cooker, and connect the plug to suitable socket. After connected, pressing the ON/OFF button , the light will shine, indicating that the power is connected normally.

2). Pressing the Power button, the Power light is on, indicating that the induction cooker enters the heating state; the default power of heating is 2000W. Adjust the power rate from level 500-3500W by press "+” or “-” 

Power level:

(500W/800W/1000W/1300W/1500W/1800W/2000W/2300W/2500W/2700W/2900W/3100W/3500W)
3). Pressing Temp button, the light of temp will shine, indicating the induction cooker is entering the state of temperature, the default temperature is 100℃, Adjust the temperature from 60℃ to 240℃ by press "+” or “-”
Temperature level:(60℃/80℃/100℃/120℃/140℃/160℃/180℃/200℃/220℃/240℃)
4). Adjust the time from 0 minute to 180 minutes by press "+” or “-”at the state of Time.

5). The induction cooker will shut off automatically if there is no any operation within 2 hours if Timer is not set above 120 minutes.

6). The temperature of accessible surfaces may be high when the appliance is operating

Warning: The appliance is equipped with an overheat protection. If the pot or pan is getting too hot, the appliance will switch off power, a buzzer sounds and on the display occurs “E1”. Should this happen, wait for some minutes and cool the appliance down. After that, the appliance works without problems.

If the induction cooker does not detect the pot, an E0 error code will appear, and then it will automatically shut down after 1 minute..

Ⅳ.Usable and Non-usable Utensils
1). Usable Pans

Steel or cast iron, enameled iron, stainless steel, Rounded-bottom stainless steel or iron pans/pots .

2). Non-usable Pans

    Heat-resistant glass, ceramic container, copper, aluminum pans/pots, flat-bottom pans/pots.
Ⅴ.How to Clean
1). Unplug and wait until the cooker is cooled down completely. Clean the cooker after using each time.

2). If the pots/pans are used without being cleaned, discoloration or cooked on stains may be caused.

3). Do not use benzine, thinner, scrubbing brush or polishing powder to clean the induction cooker.

4). Wipe using dish washing agent and damp cloth.

5). Use vacuum cleaner to suck up dirt from the air intake and exhaust vent.

6). Never run water over the unit (Water gets inside may cause malfunction).

Appliances are not intended to be operated by means of an external timer or separate remote-control system.
This appliance is intended to be used in household and similar applications such as:

– staff kitchen areas in shops, offices and other working environments;

– farm houses;

– by clients in hotels, motels and other residential type environments;

– bed and breakfast type environments.

