FED-X S/S Four Drawer Sandwich Counter - XSS7C13S2V-4D
· Cooling System: Fan forced cooling
· Temperature range: +2~+8°C
· Compressor: Cubigel
· Controller: Dixell
· Ambient Temperature: 43°C
· RH: 40%
· Stainless steel interior and exterior with rounded corners for easy cleaning
· Compatible for 7X1/3 GN Pan up to 150mm deep
· 60mm HFCs and CFCs free foam body insulation
· Tropicalised for Australian conditions
· User friendly Digital controls
· Rapid recovery rate
· Heavy duty 4 drawers 
· Ebm-papst evaporator and condenser fans
· Heavy duty castors with front wheel brakes
· Weight loading per shelf: 40kg
· Refrigerant: R290
· Display top can hold temperature for up to 4 hours from pre-chilled environment
 
2 Years Parts and Labour + 2 Years Parts only Warranty with Product Registration within 14 Days of Invoice

