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Installation,Operation & Maintenance Manual
(HC Gas R290 used)
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Safety Tips
· Position on a flat, stable surface.
· A service agent/qualified technician should carry out
installation and any repairs if required. Do not remove
any components or service panels on this product.
Consult Local and National Standards to comply with
The following:
·Health and Safety at Work Legislation
·BS EN Codes of Practice
·Fire Precautions
·IEE Wiring Regulations
·Building Regulations
· DO NOT use jet/pressure washers to clean the appliance.
· DO NOT use the appliance outside.
· DO NOT use this appliance to store medical supplies.
· DO NOT use electrical appliances inside the appliance.
(e.g. heaters, ice-cream makers etc.)
· DO NOT stand or support yourself on the base,
drawers or doors.
· DO NOT allow oil or fat to come into contact with the
plastic components or door seal. Clean immediately if
contact occurs.
· Bottles that contain a high percentage of alcohol must
be sealed and placed vertically in the refrigerator.
· Always carry, store and handle the appliance in a
vertical position and move by holding the base of the
appliance.
· Always switch off and disconnect the power supply to
the unit before cleaning.
· Keep all packing away from children. Dispose of the
packaging in accordance with the regulations of local
authorities.
· If the power cord is damaged, it must be replaced by
an agent or a recommended qualified technician in
order to avoid a hazard.
Introduction
Please take a few moments to carefully read through this
manual. Correct maintenance and operation of this
machine will provide the best possible performance from
your product.
Pack Contents
The following is included：
·Refrigerator or Freezer
·Shelf guides (2 per door)
·Shelves (1 per door)
·Instruction manual
We pride ourselves on quality and service, ensuring that 
at the time of packing the contents are supplied fully
functional and free of damage. Should you find any
damage as a result of transit, please contact your dealer
immediately.
Installation
Note: If the unit has not been stored or move in an
upright position, let it stand upright for approximately 
12 hours before operation. If in doubt allow to stand.
1. Remove the appliance from the packaging. Make
sure that all protective plastic film and coatings
are thoroughly removed from all surfaces.
2. Maintain a distance of 20 cm (7 inches) between
the unit and walls or other objects for ventilation
increase this distance if the obstacle is a heat source.

Note: Before using the appliance for the first time,
clean the shelves and interior with soapy water.


3. Set the brakes on the castors to keep the appliance
in position OR level the appliance by adjusting the screw feet.

Fitting the Shelves
1. Place one set of shelf guides on either side of the cabinet
at the desired height.
2. Slide the shelf into place.
3. Repeat for the remaining shelves.

Note: This is vital for ensuring correct drainage of condensation.

Operation 
Storing Food
To get the best result from your appliance, follow these instruction:
·Only store foodstuffs in the appliance when it has reached the correct operating temperature. 
·Do not place uncovered hot food or liquid inside the appliance.
·Warp or cover food where possible.
·Do not obstruct the fans inside the appliance.
·Avoid opening the doors for prolonged periods of time.
Turn on
1. Close the door(s) of the appliance.
2. Ensure the power switch is set to [O] and turn on at the socket.
3. Switch on the power [l]. The current temperature within the
the appliance is displayed.

Manual Defrost
The appliance will automatically run a defrost cycle every six hours.

Note: The cycle starts from the time the appliance is initially powered up.

To manually defrost the appliance:
1. Press and hold the DEFROST button for 5 seconds.
2. The defrost cycle will start immediately and the Defrost
LET illuminates. The defrost will last a maximum of 30 minutes

Note: Starting a manual defrost also resets the automatic defrost timer.
3. The next automatic defrost will start six hours after the manual 
defrost has finished.

Cleaning, Care & Maintenance
· Switch off and disconnect from the power supply before cleaning.
· Clean the interior of the appliance as often as possible.
· Do not use abrasive cleaning agents. These can leave harmful residues.
· Clean the door seal with water only.
· Always wipe dry after cleaning.
· Do not allow water used in cleaning to run through the drain hole into the evaporation pan.
· Take care when cleaning the rear of the appliance. Sharp edges can cut.
· An agent or qualified technician must carry out repairs if required.
Cleaning the Condenser
Periodically cleaning the condenser can extend the life of the
    appliance. We recommend that our agent or qualified technician clean the clean the condenser.


Troubleshooting
If your appliance develops a fault, please check the following table before making a call to your retailer.
	Fault 
	Probable Cause
	[bookmark: OLE_LINK3][bookmark: OLE_LINK4]Action

	The appliance is not working 
	The unit is not switch on
	Check the unit is plugged in correctly and switched on

	
	Plug and lead are damaged
	Call your agent or qualified technician

	
	Fuse in the plug has blown
	Replace the fuse

	
	Power supply
	Check power supply

	
	Internal wiring fault
	Call your agent or qualified technician

	The appliance turns on, but the temperature is too high/low

	Too much ice on the evaporator
	Defrost the appliance

	
	Condenser blocked with dust
	Call your agent or qualified technician

	
	Doors are not shut properly
	Check doors are shut and seals are not damaged

	
	Appliance is located near a heat source or air flow to the condenser is being interrupted 
	Move the refrigerator to a more suitable location

	
	Ambient temperature is too high
	Increase ventilation or move appliance to a cooler position

	
	Unsuitable foodstuffs are being stored in the appliance 
	Remove any excessive hot foodstuffs or blockages to the fan

	
	Appliance is overloaded
	Reduce the amount of food stored in the appliance 

	The appliance is leaking water 
	The appliance is not properly levelled
	Adjust the screw feet to level the appliance(If applicable)

	
	The discharge outside is blocked
	Clear the discharge outlet

	
	Movement of water to the drain is obstructed
	Clear the floor of the appliance (if applicable)

	
	The water container is damaged
	Call your agent or qualified technician 

	
	The drip tray is over flowing
	Empty the drip tray(if applicable)

	The appliance is unusually loud
	Loose nut/screw
	Check and tighten all nuts and screws

	
	The appliance has not been installed in a level or stable position
	Check  installation position and change if necessary







Technical Specifications (R290)
	Model
	Voltage
	Power
(W)
	Current
(A)
	Temperature
Range(℃)
	Capacity
(litres)
	Dimensions
HxWxD(mm)
	Weight
(kg)

	GX-GN2100TN-HC
	220～240V/50Hz
	215
	1.3
	-2～+8
	282
	850x1360x700
	102

	GX-GN3100TN-HC
	220～240V/50Hz
	230
	1.3
	-2～+8
	417
	850x1795x700
	121

	GX-GN4100TN-HC
	220～240V/50Hz
	345
	2.0
	-2～+8
	553
	850x2230x700
	150

	GX-GN2200TN-HC
	220～240V/50Hz
	215
	1.3
	-2～+8
	282
	950x1360x700
	103

	GX-GN3200TN-HC
	220～240V/50Hz
	230
	1.3
	-2～+8
	417
	950x1795x700
	134

	GX-GN4200TN-HC
	220～240V/50Hz
	345
	2.0
	-2～+8
	553
	950x2230x700
	159

	GX-GN2100TNG-HC
	220～240V/50Hz
	215
	1.3
	+2～+8
	282
	850x1360x700
	108

	GX-GN3100TNG-HC
	220～240V/50Hz
	230
	1.3
	+2～+8
	417
	850x1795x700
	134

	GX-GN4100TNG-HC
	220～240V/50Hz
	345
	2.0
	+2～+8
	553
	850x2230x700
	157

	GX-GN2100BT-HC
	220～240V/50Hz
	520
	3.2
	-18～-22
	282
	850x1360x700
	107

	GX-GN3100BT-HC
	220～240V/50Hz
	560
	3.4
	-18～-22
	417
	850x1795x700
	146

	GX-GN4100BT-HC
	220～240V/50Hz
	650
	4.0
	-18～-22
	553
	850x2230x700
	160

	GX-GN2200BT-HC
	220～240V/50Hz
	520
	3.2
	-18～-22
	282
	950x1360x700
	107

	GX-GN3200BT-HC
	220～240V/50Hz
	560
	3.4
	-18～-22
	417
	950x1795x700
	159

	GX-GN4200BT-HC
	220～240V/50Hz
	650
	4.0
	-18～-22
	553
	950x2230x700
	165

	GX-SNACK2100TN-HC
	220～240V/50Hz
	215
	1.3
	-2～+8
	228
	850x1360x600
	88

	Model
	Voltage
	Power
(W)
	Current
(A)
	Temperature
Range(℃)
	Capacity
(litres)
	Dimensions
HxWxD(mm)
	Weight
(kg)

	GX-SNACK3100TN-HC
	220～240V/50Hz
	230
	1.3
	-2～+8
	339
	850x1795x600
	122

	GX-SNACK4100TN-HC
	220～240V/50Hz
	345
	2
	-2～+8
	449
	850x2230x600
	143

	GX-SNACK2100TNG-HC
	220～240V/50Hz
	215
	1.3
	+2～+8
	228
	850x1360x600
	92

	GX-SNACK3100TNG-HC
	220～240V/50Hz
	230
	1.3
	+2～+8
	339
	850x1795x600
	126

	GX-SNACK4100TNG-HC
	220～240V/50Hz
	345
	2
	+2～+8
	449
	850x2230x600
	148

	GX-SNACK2200TN-HC
	220～240V/50Hz
	215
	1.3
	-2～+8
	228
	950x1360x600
	91

	GX-SNACK3200TN-HC
	220～240V/50Hz
	230
	1.3
	-2～+8
	339
	950x1795x600
	126

	GX-SNACK4200TN-HC
	220～240V/50Hz
	345
	2
	-2～+8
	449
	950x2230x600
	146

	GX-SNACK2100BT-HC
	220～240V/50Hz
	520
	3.2
	-18～-22
	228
	850x1360x600
	93

	GX-SNACK3100BT-HC
	220～240V/50Hz
	560
	3.4
	-18～-22
	339
	850x1795x600
	126

	GX-SNACK4100BT-HC
	220～240V/50Hz
	650
	4
	-18～-22
	449
	850x2230x600
	147

	GX-SNACK2200BT-HC
	220～240V/50Hz
	520
	3.2
	-18～-22
	228
	950x1360x600
	93

	GX-SNACK3200BT-HC
	220～240V/50Hz
	560
	3.4
	-18～-22
	339
	950x1795x600
	126

	GX-SNACK4200BT-HC
	220～240V/50Hz
	650
	4
	-18～-22
	449
	950x2230x600
	147

	GX-PA2100TN-HC
	220～240V/50Hz
	215
	1.3
	-2～+8
	390
	850x1510x800
	98

	GX-PA3100TN-HC
	220～240V/50Hz
	320
	1.9
	-2～+8
	580
	850x2020x800
	152

	GX-U-GN2100TN-HC
	220～240V/50Hz
	215
	1.3
	-2～+8
	172
	650x1360x700
	83

	GX-U-GN3100TN-HC
	220～240V/50Hz
	230
	1.3
	-2～+8
	255
	650x1795x700
	120

	GX-U-GN4100TN-HC
	220～240V/50Hz
	345
	2
	-2～+8
	337
	650x2230x700
	138

	GX-SH2000/700-HC
	220～240V/50Hz
	320
	1.9
	+2～+8
	282
	1085x1360x700
	125

	GX-SH2000/800-HC
	220～240V/50Hz
	320
	1.9
	+2～+8
	390
	1085x1510x800
	140

	GX-SH3000/700-HC
	220～240V/50Hz
	320
	1.9
	+2～+8
	417
	1085x1795x700
	130

	GX-SH3000/800-HC
	220～240V/50Hz
	320
	1.9
	+2～+8
	580
	1085x2020x800
	164

	GX-PZ1610TN-HC
	220～240V/50Hz
	215
	1.3
	-2～+8
	390
	1000x1515x800
	262

	GX-PZ2600TN-HC
	220～240V/50Hz
	215
	1.3
	-2～+8
	390
	1000x1510x800
	258

	GX-PZ3600TN-HC
	220～240V/50Hz
	320
	1.9
	-2～+8
	580
	1000x2020x800
	320

	GX-PZ2610TN-HC
	220～240V/50Hz
	215
	1.3
	-2～+8
	580
	1000x2025x800
	326

	GX-GN2100SALGC-HC
	220～240V/50Hz
	215
	1.3
	-2～+8
	282
	1365x1360x700
	125

	GX-GN3100SALGC-HC
	220～240V/50Hz
	230
	1.3
	-2～+8
	417
	1365x1795x700
	133

	GX-GN4100SALGC-HC
	220～240V/50Hz
	345
	2
	-2～+8
	553
	1365x2230x700
	165




Electrical Wiring
Appliances are supplied with a 3 pin, moulded, BS1363 plug and lead, with a 13 amp fuse as standard. The plug is to be 
connected to a suitable mains socket. Appliances are wired as follows:
·Live wire (coloured brown) to terminal marked L
·Neutral wire (coloured blue) to terminal marked N
·Earth wire (coloured green/yellow) to terminal marked E
All appliances must be earthed, using a dedicated earthing circuit.
If in doubt consult a qualified electrician.
Electrical isolation points must be kept clear of any obstructions. In the event of any emergency disconnection being
required they must be readily accessible.




















R290 refrigerant is used for this equipment.
[image: C:\Documents and Settings\longqing.zhong\Application Data\Tencent\Users\253130683\QQ\WinTemp\RichOle\Y_{8`8({B3Y5ZGX@}DS{G0I.png]
Caution!
Consult reprair manual/ower’s guide before attempting to install or service this product. All safety precautions must be followed. Dispose of properly in accordance with federal or local regulations. Risk of fire or explosion due to puncture of refrigerant tubing. Follow handling instructions carefully.
Danger!
Risk of fire or explosion. Flammable refrigerant used. To be repaired only by trained service personnel. Do not use mechanical devices to defrost refrigerator. Do not puncture refrigerant tubing.


[image: C:\Documents and Settings\longqing.zhong\Application Data\Tencent\Users\253130683\QQ\WinTemp\RichOle\SD2IRP8%BSCUHTC2L17@7PP.png]Disposal
EU regulations require refrigeration product to be disposed of by specialist companies who remove or recycle all glasses,
metal and plastic components.
Consult your local waste collection authority regarding disposal of your appliance. Local authorities are not obliged to 
dispose of commercial refrigeration equipment but may be able to offer advice on how to dispose of the equipment locally.
All packaging materials should be disposed of in an environmentally friendly way.
              The cardboard may be used as scrap paper. The protective foil and the foam cushions are CFD-free. 
              Do not allow children to play with the packaging and destroy plastic gags safely.


[image: C:\Documents and Settings\longqing.zhong\Application Data\Tencent\Users\253130683\QQ\WinTemp\RichOle\(BFR(@K6UCN)_NEM2%D`}ZG.png]Environmental protection
Discarded electric appliances are recyclable and should not be discarded in the domestic waste! Please actively support us in conserving resources and protecting the environment by returning this appliance to the collections centers (if available).


Compliance
Parts have undergone strict product testing in order to comply with regulatory standards and specification set by 
international, independent, and federal authorities.
Products have been approved to carry the following symbol:
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